# AC7202

# Gree Hyper Hi-Wall Inverter Air Conditioner(Heat Pump)

The new Hyper Range of heat pumps utilises Gree’s G10 inverter, this inverter module utilises a cutting edge, high speed, DSP computer chip for precise inverter control. This ensures accurate calculation and control which leads to efficient and unceasing operation.

The inverter PCB in the outdoor unit can work safely up to 85°C for greater reliability. The PCB is also coated to protect it from the ingress of moisture, dirt and dust.

The new Hyper range of outdoor units feature Gold Fin coating on the outdoor coil. This improves efficiency by accelerating the defrost process and offers greater resistant to corrosive elements. Gold fin coils perform 20x better under salt spray testing than Blue Fin Coils.

All Gree hi-walls come with an industry leading “Six Year, Parts and Labour Warranty”. And there are no strings attached, if your installer is industry qualified that’s ok by Gree.

All motors and fan motors are DC for greater energy efficiency and better performance.

**Warranty:**

* 12 years warranty
* 4 years pcb card warranty
* SKU: F01000000084
* Categories: [AC](https://www.dawlance.com.pk/product-category/ac/), [Inverter Series AC](https://www.dawlance.com.pk/product-category/ac/inverter-series/)

**Technical Specs**

**Comfort**

* Wired Controller
* Dehumidifying
* Trubo Button
* Dred
* Golden Fin
* LED Display
* Healthy Filters

**Energy Efficiency**

* EER – 5.36
* Cooler Liquid – R32
* Energy in Heating(KW) – 2.6-3.15

**Silence**

* Noise Level DB - 44
* Outdoor DB - 57

**Air Quality**

* Air Flow rate m3/hr - 231
* Other

 Sleep mode

 Removable / Washable Panel

 Self Diagnosis

 Turbo Mode

* +  Memory Function
  +  Anti Rust Outdoor Casing
  +  Moisture Removal L/h:1

**Dimension**

* Outdoor Unit(WxDxH)mm – 798×295×222
* Indoor Unit(WxDxH)mm – 899×596×378

**Capacity**

* Cooling Capacity (Btu / h) – 204000 BTU / h
* Voltage Range – 210 - 240