# HPU-24HDZ/012DC(G)

# Yunding Inverter(DC)

Dirt accumulates on the evaporator of the air conditioner during its operation, the dirty evaporator facilitates bacterial growth and affect the quality of air out and the health of our body, our patent Cold Expansion Technology freezes the surface with moisture in the air and removes the dirt in defrosting. Supper long vertical blowing cabinet design , supplying fast comfort for big space. Super quiet operation for noise less comfortable sleep, lowest Noise level low up to 26[db(A)]

**Warranty:**

* 1 year parts
* 5 years Compressor

**Technical Specs**

**Comfort**

* Wired Controller
* Dehumidifying
* Trubo Button
* Dred
* Golden Fin
* LED Display
* Healthy Filters

**Energy Efficiency**

* EER – 8.6
* Cooler Liquid – R410A
* Energy in Heating(KW) – 3.27-12.13

**Silence**

* Noise Level DB - 45
* Outdoor DB - 56

**Air Quality**

* Air Flow rate m3/hr - 1200
* Other

 Sleep mode

 Removable / Washable Panel

 Self Diagnosis

 Turbo Mode

* +  Memory Function
  +  Anti Rust Outdoor Casing
  +  Moisture Removal L/h:1

**Dimension**

* Outdoor Unit(WxDxH)mm – 1085x487x84
* Indoor Unit(WxDxH)mm – 3377x407x1810

**Capacity**

* Cooling Capacity (Btu / h) – 122050 BTU / h
* Voltage Range – 820 - 2670