# HPU-24HYD/012DC(G)

# Yunding Inverter(DC)

Absorb 20% more wind by its double air Vents and evaporators to balance the temperature quickly and and for long time. Dirt accumulates on the evaporator of the air conditioner during its operation, the dirty evaporator facilitates bacterial growth and affect the quality of air out and the health of our body, our patent Cold Expansion Technology freezes the surface with moisture in the air and removes the dirt in defrosting. Smart Air Quality Sensor deducts the pollution in the Air, its Supper IFD filter automatically purify the room Air.

**Warranty:**

* 1 year parts
* 5 years Compressor

**Technical Specs**

**Comfort**

* Wired Controller
* Dehumidifying
* Trubo Button
* Dred
* Golden Fin
* LED Display
* Healthy Filters

**Energy Efficiency**

* EER – 9.6
* Cooler Liquid – R410A
* Energy in Heating(KW) – 2.6-3.15

**Silence**

* Noise Level DB - 42
* Outdoor DB - 69

**Air Quality**

* Air Flow rate m3/hr - 1200
* Other

 Sleep mode

 Removable / Washable Panel

 Self Diagnosis

 Turbo Mode

* +  Memory Function
  +  Anti Rust Outdoor Casing
  +  Moisture Removal L/h:1

**Dimension**

* Outdoor Unit(WxDxH)mm – 798×295×222
* Indoor Unit(WxDxH)mm – 899×596×378

**Capacity**

* Cooling Capacity (Btu / h) – 24000 BTU / h
* Voltage Range – 300 - 310